August 2018

|  |  |  |
| --- | --- | --- |
|  |  |  |

**Product Guide Specification**

Specifier Notes: This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on *MasterFormat 2016* and *The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy.*

The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code. Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement. Coordinate this section with other specification sections and the Drawings. Delete all “Specifier Notes” after editing this section.

**Section 28 00 00: Electronic Safety and Security**

**Section 28 05 00: Common Work Results For Electronic Safety and Security**

**Section 28 05 19.11: Digital Video Recorders**

**1080p H.265 HDCVI PENTA-BRID DVR**

1. **– GENERAL**
	1. SUMMARY
		1. Section Includes
			1. Section 28 05 23: Storage Area Network Electronic Safety and Security
			2. Section 28 05 25: Cloud Based Storage for Electronic Safety and Security
			3. Section 28 05 29: Storage Management Software for Electronic Safety and Security
			4. Section 28 05 31: Communications Equipment for Electronic Safety and Security
		2. Related Sections
			1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].

\*\*\*\*\*\*\*\*\*\*Specifier’s note: Include those standards referenced elsewhere in this SECTION.

* 1. REFERENCES
		1. Federal Communications Commission (FCC) ([www.fcc.gov](http://www.fcc.gov))
			1. CFR 47 FCC Part 15 Subpart B
		2. Underwriters Laboratories, Inc. (UL) (www.ul.com)
			1. UL 60950-1
		3. European Standards
			1. EN 55032
			2. EN 50130
			3. EN61000-3-2
			4. EN 6100-3-3
			5. EN 55024:2010
			6. EN 60950-1
			7. IEC 60950-1
	2. SYSTEM DESCRIPTION
		1. Section Includes
			1. Digital Video Recorders
		2. Performance Requirements
			1. The 1080p Penta-brid HDCVI DVR shall be an embedded processer with embedded Linux operating system to record video from HDCVI, AHD, TVI, CVBS, and IP video sources.
			2. The 1080p Penta-brid HDCVI DVR shall be capable of storing up to 80 TB of data from a total of 32 analog and IP camera video inputs with up to 8 MP resolution for each IP input.
			3. The 1080p Penta-brid HDCVI DVR shall offer a maximum recording resolution of 5 M-N at 20 fps.
			4. The 1080p Penta-brid HDCVI DVR shall use the Smart H.265+ and the Smart H.264+ Video compression protocols.
			5. The 1080p Penta-brid HDCVI DVR shall have a maximum incoming bandwidth of 128 Mbps.
			6. The 1080p Penta-brid HDCVI DVR shall automatically detect and recognize the transmission protocol (HDCVI, AHD, TVI or CVBS) of each attached analog camera.
			7. The 1080p Penta-brid HDCVI DVR shall offer a selection of built-in recording options and schedules.
			8. The 1080p Penta-brid HDCVI DVR shall offer a smart search function to search a specific region of the playback video.
			9. The 1080p Penta-brid HDCVI DVR shall come in a 2U-high casing.
	3. SUBMITTALS

* + 1. Submit under provisions of Section [01 33 00.]
		2. Product Data:
			1. Manufacturer’s data, user and installation manuals for all equipment and software programs including computer equipment and other equipment required for complete video management system.
		3. Dimensional Drawings; include
			1. Overall device dimensions.
			2. Dimensions specific for installation.
		4. Closeout Submittals
			1. User manual.
			2. Parts list.
			3. Maintenance requirements.
	1. QUALITY ASSURANCE
		1. Manufacturer:
			1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.
		2. Video Surveillance System:
			1. List certifying bodies (UL, CSA, etc.)
			2. Provide evidence of compliance upon request.
		3. Installer:
			1. Minimum of [5] years of experience installing Video Surveillance System.
	2. DELIVERY, STORAGE AND HANDLING
		1. Comply with requirements of Section 01 60 00.
		2. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels.
		3. Protect store materials from environmental and temperature conditions following manufacturer’s instructions.
		4. Handle and operate products and systems according to manufacturer’s instructions.
	3. WARRANTY
		1. Provide manufacturer’s warranty covering [2] years for replacement and repair of defective equipment. Warranty varies country to country.
	4. MAINTENANCE
		1. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.
		2. Provide factory direct technical support via phone and e-mail.
1. **– PRODUCTS**
	1. MANUFACTURERS
		1. [Acceptable Manufacturer:

Dahua Technology USA Inc.

23 Hubble, Irvine, CA 92618

Tel: (949) 679-7777

Fax: (949) 679-5760

Email: sales.usa@global.dahuatech.com]

* + 1. Substitutions: [Not permitted.] [Under provisions of Division 1.]
			1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
			2. [Proposed substitutions must provide a line-by-line compliance documentation.]
	1. 1080p H.265 HDCVI PENTA-BRID DVR [X58A5S]

		1. General Characteristics:
			1. The 1080p Penta-brid HDCVI DVR shall be an embedded processer with embedded Linux operating system to record video from HDCVI, AHD, TVI, CVBS, and IP video sources.
			2. The 1080p Penta-brid HDCVI DVR shall be capable of storing up to 80 TB of data from a total of 32 analog and IP camera video inputs with up to 8 MP resolution for each IP input.
			3. The 1080p Penta-brid HDCVI DVR shall offer a maximum recording resolution of 5 M-N at 20 fps.
			4. The 1080p Penta-brid HDCVI DVR shall use the Smart H.265+ and the Smart H.264+ Video compression protocols.
			5. The 1080p Penta-brid HDCVI DVR shall have a maximum incoming bandwidth of 128 Mbps.
			6. The 1080p Penta-brid HDCVI DVR shall automatically detect and recognize the transmission protocol (HDCVI, AHD, TVI or CVBS) of each attached analog camera.
			7. The 1080p Penta-brid HDCVI DVR shall offer a selection of built-in recording options and schedules.
			8. The 1080p Penta-brid HDCVI DVR shall offer a smart search function to search a specific region of the playback video.
			9. The 1080p Penta-brid HDCVI DVR shall come in a 2U-high casing.
			10. The 1080p Penta-brid HDCVI DVR shall be powered by a 100 VAC to 240 VAC, 50/60 Hz power supply and consume less than 35 W of power.
		2. Display
			1. The 1080p Penta-brid HDCVI DVR shall offer two (2) HDMI, one (1) VGA, and one (1) BNC video output interfaces. The HDMI ports shall provide output up to 3840 x 2160.
			2. The 1080p Penta-brid HDCVI DVR shall offer display resolutions of: 3480 x 2160, 2560 x 1440, 1920 × 1080, 1280 × 1024, 1280 × 720.
			3. The 1080p Penta-brid HDCVI DVR shall offer 1/4/8/9/16/25/36 multi-screen display.
			4. The 1080p Penta-brid HDCVI DVR shall offer an on-screen display that lists the camera title, time, video loss indication, camera lock indication, motion detection, and recording indicator.
		3. Video Detection and Alarm
			1. The 1080p Penta-brid HDCVI DVR shall offer the following trigger events: recording, PTZ, tour, alarm our, video push, Email, FTP, snapshot, buzzer, and screen tips.
			2. The 1080p Penta-brid HDCVI DVR shall be capable of detecting motion (396 zones), video loss, tampering, and diagnosis.
			3. The 1080p Penta-brid HDCVI DVR shall offer 16 alarm inputs and six (6) relay outputs.
		4. Interface
			1. The 1080p Penta-brid HDCVI DVR shall have 32 analog (HDCVI, AHD, TVI or CVBS) camera inputs.
			2. The 1080p Penta-brid HDCVI DVR shall allow all 32 to record IP cameras or any combination of analog and IP cameras that total 32 video inputs.
			3. The 1080p Penta-brid HDCVI DVR shall offer two (2) USB 2.0 auxiliary ports and two (2) USB 3.0 auxiliary ports.
			4. The 1080p Penta-brid HDCVI DVR shall offer one serial interface that connects to one (1) of the following protocols:
				1. RS232: for PC communication or keyboard control
				2. RS22: for PTZ control.
				3. RS485: for PTZ control.
			5. The 1080p Penta-brid HDCVI DVR shall offer 16 BNC audio input channels and one (1) BNC audio output channel.
			6. The 1080p Penta-brid HDCVI DVR shall allow two-way talk with one (1) BNC microphone input connector and one (1) BNC microphone output connector.
		5. Storage
			1. The 1080p Penta-brid HDCVI DVR shall come with eight (8) SATA ports that can each support a 10 TB HDD.
		6. Playback and Backup
			1. The 1080p Penta-brid HDCVI DVR shall support output to 1/4/9/16 playback devices.
			2. The 1080p Penta-brid HDCVI DVR shall allow recorded video searches by time/date, motion detection event, Exact Search, and Smart Search.
			3. The 1080p Penta-brid HDCVI DVR shall offer the following playback functions: Play, Pause, Stop, Rewind, Fast Play, Slow Play, Next File, Previous File, Next Camera, Previous Camera, Full Screen, Repeat, Shuffle, Backup Selection, and Digital Zoom.
			4. The 1080p Penta-brid HDCVI DVR shall allow data backup via a USB device or another network.
		7. Recording
			1. The 1080p Penta-brid HDCVI DVR shall employ the Smart H.265+ and the Smart H.264+ video compression protocols.
			2. The 1080p Penta-brid HDCVI DVR shall offer video recording resolutions of
			5 M-N, 4 M-N, 1080p, 1080N, 720p, 960H, D1, and CIF.
			3. The 1080p Penta-brid HDCVI DVR shall allow a bit rate of 32 Kbps to
			6144 Kbps per channel.
			4. The 1080p Penta-brid HDCVI DVR shall offer dual recording at the following rates:
				1. Main Stream:

Channels 1 and 2: 5 M-N at 20 fps

Channels 3 to 32: 4 M-N at 30 fps

* + - * 1. Sub Stream: D1 or CIF at 30 fps
			1. The 1080p Penta-brid HDCVI DVR shall offer the following built-in recording modes:
				1. Manual
				2. Schedule, regular or continuous
				3. Video Detection: Motion Detection, Video Loss, Tampering
				4. Alarm
				5. Stop
			2. The 1080p Penta-brid HDCVI DVR shall offer a recording interval between 1 minute and 60 minutes. In addition, the 1080p Penta-brid HDCVI DVR shall offer a pre-record interval of between 1 second to 30 seconds, and a post-record interval of between 10 seconds to 300 seconds.
			3. The 1080p Penta-brid HDCVI DVR shall be capable of recording from third-party devices, including: Dahua, Arecont Vision, AXIS, Bosch, Brickcom, Canon, CP Plus, Dynacolor, Honeywell, Panasonic, Pelco, Samsung, Sanyo, Sony, Videotec, and Vivotek.
		1. IP Connectivity
			1. The 1080p Penta-brid HDCVI DVR shall allow full control and configuration capabilities via a TCP/IP network.
			2. The 1080p Penta-brid HDCVI DVR shall offer two RJ-45 ports (1000 Mbps).
			3. The 1080p Penta-brid HDCVI DVR shall support a maximum of 128 user access points.
			4. The 1080p Penta-brid HDCVI DVR shall conform to the ONVIF 16.12 and to the CGI standards.
			5. The 1080p Penta-brid HDCVI DVR shall offer the following audio compression standards:
				1. AAC (first channel)
				2. G.711A
				3. G.711U
				4. PCM
			6. The 1080p Penta-brid HDCVI DVR shall support the IPv6 internet-layer protocol for packet switched internetworking across multiple IP networks.
			7. The 1080p Penta-brid HDCVI DVR shall support the IPv4/ IPv6, HTTP, HTTPS, SSL, TCP/IP, UDP, UPnP, ICMP, IGMP, SNMP, RTSP, RTP, SMTP, NTP, DHCP, DNS, PPPOE, DDNS, FTP, IP Filter, QoS, Bonjour, and 802.1x.
			8. The 1080p Penta-brid HDCVI DVR shall support the IOS and the Android mobile operating systems.
		2. Intelligent Video System
			1. The 1080p Penta-brid HDCVI DVR shall offer a built-in Intelligent Video System to provide advanced analytics for a scene transmitted from a camera connected to the DVR.
			2. The Intelligent Video System shall offer intelligent video analytics built-in to the 1080p Penta-brid HDCVI DVR.
			3. The Intelligent Video System shall be capable of processing and analyzing video within the camera itself, with no extra hardware required.
			4. The Intelligent Video System shall trigger an alarm and take a defined action for the following events:
				1. Premium Features

Tripwire: a target crosses a user-defined line (channels 1 through 16).

Intrusion: a target enters or exits a defined perimeter (channels 1 through 16).

Abandoned/Missing Object: a target leaves an object in a designated area, or a target removes and object from the same designated area channels 1 and 2).

* + - * 1. Advanced Features

Facial Detection: detects and captures a snapshot of a human face in a defined area within a scene (analog channel 1).

* + 1. Installation Requirements
			1. The 1080p Penta-brid HDCVI DVR shall be capable of operating in temperatures between -10°C to +55°C (+14°F to +131°F).
			2. The 1080p Penta-brid HDCVI DVR shall receive power from a 100 to 240 VAC, 50/60 Hz power source and consume less than 35 W of power.
1. **– EXECUTION**
	1. EXAMINATION
		1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
		2. Do not begin installation until unacceptable conditions are corrected.
	2. PREPARATION
		1. Protect devices from damage during construction.
	3. INSTALLATION
		1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
		2. Perform installation with qualified service personnel.
		3. Install devices in accordance with the National Electrical Code or applicable local codes.
		4. Ensure selected location is secure and offers protection from accidental damage.
		5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
	4. FIELD QUALITY CONTROL
		1. Test snugness of mounting screws of all installed equipment.
		2. Test proper operation of all video system devices.
		3. Determine and report all problems to the manufacturer’s customer service department.
	5. ADJUSTING
		1. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
		2. Make any adjustment of camera settings to comply with specific customer’s need.
	6. DEMOSTRATION
		1. Demonstrate at final inspection that video management system and devices functions properly.

END OF SECTION