AUGUST 2021

|  |  |  |
| --- | --- | --- |
|  |  |  |

**Product Guide Specification**

Specifier Notes: This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on *MasterFormat 2016* and *The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy.*

The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code. Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement. Coordinate this section with other specification sections and the Drawings. Delete all “Specifier Notes” after editing this section.

**Section 28 21 00: Video Surveillance**

**Section 28 21 13: IP Cameras**

**4 MP STARLIGHT NETWORK EYEBALL CAMERA**

1. **– GENERAL**
	1. SUMMARY
		1. Section Includes
			1. Section 28 21 17: Video Surveillance – Surveillance Cameras – Camera Housings
			2. Section 28 21 19: Video Surveillance – Surveillance Cameras – Camera Mounts
			3. Section 28 21 21: Video Surveillance – Surveillance Cameras – Illuminators
			4. Section 28 27 00: Video Surveillance – Video Surveillance Sensors
		2. Related Sections
			1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].

\*\*\*\*\*\*\*\*\*\*Specifier’s note: Include those standards referenced elsewhere in this SECTION.

* 1. REFERENCES
		1. Federal Communications Commission (FCC) ([www.fcc.gov](http://www.fcc.gov))
			1. FCC Part 15 Subpart B
		2. Underwriters Laboratories, Inc. (UL) (www.ul.com)
			1. UL60950-1
			2. CAN/CSA C22.2 No.60950-1-07
		3. European Standards
			1. EN62368-1
		4. HD standards
			1. Complies with the SMPTE 274M-2008 Standard in:
				1. Resolution: 1920x1080
				2. Scan: Progressive
				3. Color representation: complies with ITU-R BT.709
				4. Aspect ratio: 16:9
				5. Frame rate: 25 and 30 frames/s
			2. Complies with the 296M-2001 Standard in:
				1. Resolution: 1280x720
				2. Scan: Progressive
				3. Color representation: complies with ITU-R BT.709
				4. Aspect ratio: 16:9
				5. Frame rate: 25, 30, 50 and 60 frames/s
				6. Interference-Causing Equipment Standards
	2. SYSTEM DESCRIPTION
		1. Section Includes
			1. Video Surveillance – Surveillance Cameras – IP Cameras
		2. Performance Requirements
			1. The 4 MP Starlight Camera shall be a full-featured network eyeball camera designed for discrete video surveillance applications in indoor and outdoor environments.
			2. The 4 MP Starlight Camera shall use a high performance 1/3-in. 4 MP Progressive-scan CMOS sensor.
			3. The 4 MP Starlight Camera shall utilize Starlight Technology with a high-performance sensor to deliver color images in low-light environments.
			4. The 4 MP Starlight Camera shall offer IR LEDs to produce images in total darkness.
			5. The 4 MP Starlight Camera shall offer tripwire and intrusion analytics.
			6. The 4 MP Starlight Camera shall include a built-in microphone.
			7. The 4 MP Starlight Camera shall provide direct network connection using Smart H.265+, H.265, Smart H.264+, H.264, or MJPEG compression and bandwidth throttling to efficiently manage bandwidth and storage requirements while delivering outstanding image quality.
			8. The 4 MP Starlight Camera shall support the following dual, redundant power options:
				1. 12 VDC
				2. PoE (IEEE 802.3af, class 0)
				3. The 4 MP Starlight Camera shall default to use power from the PoE power supply, if connected.
				4. The 4 MP Starlight Camera shall reboot and switch to the 12 VDC power supply if power from the PoE power supply is lost.
			9. The 4 MP Starlight Camera shall offer True Wide Dynamic Range for clear images in extreme high-contrast environments.
			10. The 4 MP Starlight Camera shall offer two (2) separate and configurable streams.
			11. The 4 MP Starlight Camera shall have a 2.8 mm fixed lens.
			12. The 4 MP Starlight Camera shall combine temperature-tolerant components with a waterproof enclosure to ensure flawless operation in temperatures as low as –40° C (–40° F).
			13. The 4 MP Starlight Camera housing shall conform to the IP67 Ingress Protection standard.
	3. SUBMITTALS

 Submit under provisions of Section [01 33 00.]

* + 1. Product Data:
			1. Manufacturer’s data, user and installation manuals for all equipment and software programs including computer equipment and other equipment required for complete video management system.
		2. Dimensional Drawings; include
			1. Overall device dimensions.
			2. Dimensions specific for installation.
		3. Closeout Submittals
			1. User manual.
			2. Parts list.
			3. Maintenance requirements.
	1. QUALITY ASSURANCE
		1. Manufacturer:
			1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.
		2. Video Surveillance System:
			1. List certifying bodies (UL, CSA, etc.)
			2. Provide evidence of compliance upon request.
		3. Installer:
			1. Minimum of [5] years of experience installing Video Surveillance System.
	2. DELIVERY, STORAGE AND HANDLING
		1. Comply with requirements of Section 01 60 00.
		2. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels.
		3. Protect store materials from environmental and temperature conditions following manufacturer’s instructions.
		4. Handle and operate products and systems according to manufacturer’s instructions.
	3. WARRANTY
		1. Provide manufacturer’s warranty covering [5] years for replacement and repair of defective equipment. Warranty varies country to country.
	4. MAINTENANCE
		1. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.
		2. Provide factory direct technical support via phone and e-mail.
1. **– PRODUCTS**
	1. MANUFACTURERS
		1. [Acceptable Manufacturer:

Dahua Technology USA Inc.

15245 Alton Pkwy, #100, Irvine, CA, 92618

Tel: (949) 679-7777

Fax: (949) 679-5760

Email: sales.usa@global.dahuatech.com]

* + 1. Substitutions: [Not permitted.] [Under provisions of Division 1.]
			1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
			2. [Proposed substitutions must provide a line-by-line compliance documentation.]
	1. 4 MP STARLIGHT FIXED EYEBALL NETWORK CAMERA N42BJ62

		1. General Characteristics:
			1. The 4 MP Starlight Camera shall be a full-featured network eyeball camera designed for discrete video surveillance applications in indoor and outdoor environments.
			2. The 4 MP Starlight Camera shall use a high performance 1/3-in. 4 MP Progressive-scan CMOS sensor.
			3. The 4 MP Starlight Camera shall utilize Starlight Technology with a high-performance sensor to deliver color images in low-light environments.
			4. The 4 MP Starlight Camera shall offer a IR LEDs to produce images in total darkness.
			5. The 4 MP Starlight Camera shall offer tripwire and intrusion analytics.
			6. The 4 MP Starlight Camera shall include a built-in microphone.
			7. The 4 MP Starlight Camera shall provide direct network connection using Smart H.265+, H.265, Smart H.264+, H.264, or MJPEG compression and bandwidth throttling to efficiently manage bandwidth and storage requirements while delivering outstanding image quality.
			8. The 4 MP Starlight Camera shall support the following dual, redundant power options:
				1. 12 VDC
				2. PoE (IEEE 802.3af, class 0)
				3. The 4 MP Starlight Camera shall default to use power from the PoE power supply, if connected.
				4. The 4 MP Starlight Camera shall reboot and switch to the 12 VDC power supply if power from the PoE power supply is lost.
			9. The 4 MP Starlight Camera shall offer True Wide Dynamic Range for clear images in extreme high-contrast environments.
			10. The 4 MP Starlight Camera shall offer two (2) separate and configurable streams.
			11. The 4 MP Starlight Camera shall have a 2.8 mm fixed lens.
			12. The 4 MP Starlight Camera shall combine temperature-tolerant components with a waterproof enclosure to ensure flawless operation in temperatures as low as –40° C (–40° F).
			13. The 4 MP Starlight Camera housing shall conform to the IP67 Ingress Protection standard.
		2. Imaging
			1. The 4 MP Starlight Camera shall offer a 1/3-in. 4 MP Progressive-scan CMOS imager.
			2. The 4 MP Starlight Camera shall offer an effective number of pixels of 2688(H) x 1520(V) effective picture elements.
			3. The 4 MP Starlight Camera shall offer a 2.8 mm fixed lens.
			4. The 4 MP Starlight Camera shall have a horizontal angle of 102° and a vertical angle of 55°.
			5. The 4 MP Starlight Camera shall offer a maximum aperture of F1.6.
			6. The 4 MP Starlight Camera shall produce a color image with a minimum scene illumination of 0.008 lux at F1.6.
		3. Illumination
			1. The 4 MP Starlight Camera shall have two (2) IR LEDs.
			2. The 4 MP Starlight Camera shall offer an LED distance of up to 30.0 m
			(98.43 ft).
		4. Video Characteristics
			1. The 4 MP Starlight Camera shall offer CBR/VBR bit rate control.
			2. The 4 MP Starlight Camera shall offer the following video compression protocols
				1. H.265 (12 K to 6144 Kbps)
				2. H.264 (32 K to 6144 Kbps)
			3. The 4 MP Starlight Camera shall offer Smart H.265+ and Smart H.264+ video compression protocols.
			4. The 4 MP Starlight Camera shall offer BLC, HLC, SSA, and True WDR modes of backlight compensation.
			5. The 4 MP Starlight Camera shall offer Auto, Natural, Street Lamp, Outdoor, Manual, and Regional Custom White Balance modes.
			6. The 4 MP Starlight Camera shall offer 3D DNR noise reduction.
			7. The 4 MP Starlight Camera shall offer motion detection (four zones) and region of interest (four zones) controls.
			8. The 4 MP Starlight Camera shall offer four (4) privacy masking areas.
			9. The 4 MP Starlight Camera shall offer a Flip mode at 0°, 90°, 180°, and 270°.
		5. Streaming Capability
			1. The 4 MP Starlight Camera shall generate full 4 MP
			(2688 x 1520 pixels) at 20 fps resolution using Smart H.265+ compression.
			2. The 4 MP Starlight Camera shall offer Unicast and Multicast streaming methods.
			3. The 4 MP Starlight Camera shall offer the following resolutions:
				1. 2688 x 1520
				2. 2560 x 1440
				3. 2304 x 1296
				4. 1080p (1920 x 1080)
				5. 1.3 MP (1280 x 960)
				6. 720p (1280 x 720)
				7. D1 (704 x 480)
				8. VGA (640 x 480)
				9. CIF (352 x 240)
			4. The 4 MP Starlight Camera shall generate three streams at the following maximum resolutions:
				1. Main Stream: 2688 x 1520 at 20 fps or 2560 x 1440 at 30 fps
				2. Sub Stream 1: D1 at 30 fps
		6. IP Connectivity
			1. The 4 MP Starlight Camera shall allow full camera control and configuration capabilities via a TCP/IP network.
			2. The 4 MP Starlight Camera shall deliver 4 MP video, at rates up to 30 frames per second via TCP/IP over an RJ-45 (10/100 Base-T) connection.
			3. The 4 MP Starlight Camera shall conform to the ONVIF Profile S, G, and T.
			4. The 4 MP Starlight Camera shall offer Quality of Service (QoS) configuration options.
			5. The 4 MP Starlight Camera shall support the IPv6 internet-layer protocol for packet switched internetworking across multiple IP networks.
			6. The 4 MP Starlight Camera shall offer local and network storage options that include: MicroSD, Network Attached Storage (NAS), and recording to a local PC for instant recording.
			7. The 4 MP Starlight Camera shall support the following protocols: IPv4/ IPv6, HTTP, HTTPS, SSL, TCP/IP, UDP, UPnP, ICMP, IGMP, SNMP, RTSP, RTP, SMTP, NTP, DHCP, DNS, PPPOE, DDNS, FTP, IP Filter, QoS, Bonjour, and 802.1x.
			8. The 4 MP Starlight Camera shall support the DSS management software and the DMSS mobile application.
			9. The 4 MP Starlight Camera shall support the Android and the IOS mobile operating systems.
		7. Intelligent Video System
			1. The 4 MP Starlight Camera offer a built-in Intelligent Video System to provide advanced analytics for any scene.
			2. The Intelligent Video System shall offer intelligent video analytics built-in to the camera.
			3. The Intelligent Video System shall be capable of processing and analyzing video within the camera itself, with no extra hardware required.
			4. The Intelligent Video System shall trigger an alarm and take a defined action for the following events:
				1. Standard Features

Tampering with the camera.

Error writing to an onboard Micro SD Card.

Error sending or receiving data over the network.

Unauthorized access to the camera.

* + - * 1. Premium Features

Tripwire: A target crosses a user-defined line.

Intrusion: A target enters or exits a defined perimeter.

* + 1. Installation Requirements
			1. The 4 MP Starlight Camera shall be capable of operating in an outdoor environment within a temperature range of –40° C to +60° C
			(–40° F to +140° F).
			2. The 4 MP Starlight Camera shall accept power, transmit video, and accept control via an Ethernet connection.
			3. The 4 MP Starlight Camera shall support the following dual, redundant power options:
				1. 12 VDC
				2. PoE (IEEE 802.3af, class 0)
				3. The 4 MP Starlight Camera shall default to use power from the PoE power supply, if connected.
				4. The 4 MP Starlight Camera shall reboot and switch to the 12 VDC power supply if power from the PoE power supply is lost.
		2. Housing Options
			1. The 4 MP Starlight Camera shall be offered in a metal housing.
			2. The 4 MP Starlight Camera housing shall conform to the IP67 Ingress Protection standard.
	1. ACCESSORIES
		1. The 4 MP Starlight Camera shall offer the following optional accessories:
			1. [Junction box.]
			2. [Corner mount.]
			3. [Wall mount.]
			4. [Pole mount.]
			5. [Ceiling mount.]
			6. [12 VDC, 1 A Power Adapter.]
1. **– EXECUTION**
	1. EXAMINATION
		1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
		2. Do not begin installation until unacceptable conditions are corrected.
	2. PREPARATION
		1. Protect devices from damage during construction.
	3. INSTALLATION
		1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
		2. Perform installation with qualified service personnel.
		3. Install devices in accordance with the National Electrical Code or applicable local codes.
		4. Ensure selected location is secure and offers protection from accidental damage.
		5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
	4. FIELD QUALITY CONTROL
		1. Test snugness of mounting screws of all installed equipment.
		2. Test proper operation of all video system devices.
		3. Determine and report all problems to the manufacturer’s customer service department.
	5. ADJUSTING
		1. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
		2. Make any adjustment of camera settings to comply with specific customer’s need.
	6. DEMOSTRATION
		1. Demonstrate at final inspection that video management system and devices functions properly.

END OF SECTION